From ef0b7a1582eb35581775fd82182d2415d5fb89df Mon Sep 17 00:00:00 2001
From: Alexander Tuneskog <aletu130@student.liu.se>
Date: Thu, 10 Oct 2019 11:13:27 +0200
Subject: =?UTF-8?q?=C3=84ndrade=20sm=C3=A5stavelser=20i=20Kallibrering.tex?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 Dokument/Designspec/events/Kallibrering.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'Dokument/Designspec/events/Kallibrering.tex')

diff --git a/Dokument/Designspec/events/Kallibrering.tex b/Dokument/Designspec/events/Kallibrering.tex
index 4ab48fe..2c29dc0 100644
--- a/Dokument/Designspec/events/Kallibrering.tex
+++ b/Dokument/Designspec/events/Kallibrering.tex
@@ -5,7 +5,7 @@ kalibreras. Enligt kravsspecifikation punkt 22 får det inte genomföras fler ä
 Kalibreringsvarven kommer att behöva ta hänsyn till tre moment. Det första momentet är att
 identifiera vilken konstant en bil behöver, det andra momentet är att optimera för
 gemensam varvtid och det tredje är att optimera den valda varvtiden. Vid
-kalibreringsvarven kommer den mesta kalibreringen göras för att identifiera
+kalibreringsvarven kommer den mest omfattande kalibreringen att göras med syfte att identifiera
 vilken konstant en bil har. Med indata kommer programmet kunna göra beräkningar
 om vilka konstanter som ska användas till vardera bilars körning. Under
 kalibreringsvarven är det också viktigt att anpassa båda bilarnas varvtid med
-- 
cgit v1.2.1

