From 1f40e49f77cd17707b8c73c33ba0f06a4cbef6a7 Mon Sep 17 00:00:00 2001
From: Alexander Tuneskog <aletu130@student.liu.se>
Date: Tue, 8 Oct 2019 16:32:40 +0200
Subject: =?UTF-8?q?=C3=84ndarde=20ett=20stavfel=20i=20manuellk=C3=B6rning?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 Dokument/Designspec/events/manuell.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'Dokument/Designspec/events/manuell.tex')

diff --git a/Dokument/Designspec/events/manuell.tex b/Dokument/Designspec/events/manuell.tex
index eae1ff0..41fc062 100644
--- a/Dokument/Designspec/events/manuell.tex
+++ b/Dokument/Designspec/events/manuell.tex
@@ -1,6 +1,6 @@
 Enligt kravspecifikationens punkt 12 ska de två olika banorna delas upp så att
 ena banan styrs autonomt och den andra manuellt.  Den manuella delen ska bli
-hjälpt av programmet för att underläta körning vid händelse av driftfall samt
+hjälpt av programmet för att underlätta körning vid händelse av driftfall samt
 uppvärmning av banan.  Detta ska uppnås genom att jämföra vilken hastighet bilen
 erhåller i ett visst segment styrt av vilken spänningspåläggning som verkar på
 bilen.  Sedan ska programmet jämföra hastigheten med en tidigare föreslagen
-- 
cgit v1.2.1

