From a2026e7154fd277add65e0ad0f5d22227b259a64 Mon Sep 17 00:00:00 2001
From: Albin <albwa833@student.liu.se>
Date: Tue, 8 Oct 2019 21:02:13 +0200
Subject: =?UTF-8?q?Korrekturl=C3=A4ste=20och=20=C3=A4ndrade=20lite.=20Fram?=
 =?UTF-8?q?f=C3=B6rallt=20i=20"missade=20givare"=20och=20"manuell".?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 Dokument/Designspec/events/manuell.tex | 7 +------
 1 file changed, 1 insertion(+), 6 deletions(-)

(limited to 'Dokument/Designspec/events/manuell.tex')

diff --git a/Dokument/Designspec/events/manuell.tex b/Dokument/Designspec/events/manuell.tex
index 41fc062..4bb4bee 100644
--- a/Dokument/Designspec/events/manuell.tex
+++ b/Dokument/Designspec/events/manuell.tex
@@ -1,8 +1,3 @@
 Enligt kravspecifikationens punkt 12 ska de två olika banorna delas upp så att
-ena banan styrs autonomt och den andra manuellt.  Den manuella delen ska bli
-hjälpt av programmet för att underlätta körning vid händelse av driftfall samt
-uppvärmning av banan.  Detta ska uppnås genom att jämföra vilken hastighet bilen
-erhåller i ett visst segment styrt av vilken spänningspåläggning som verkar på
-bilen.  Sedan ska programmet jämföra hastigheten med en tidigare föreslagen
-hastighet och sedan modifiera en konstant för att matcha det önskade värdet.
+ena banan styrs autonomt och den andra manuellt.  
 
-- 
cgit v1.2.1

