From ab43d36925a699d43f8b9fecf58e80ca67d4775d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?David=20Thor=C3=A9n?= <davth346@student.liu.se>
Date: Sun, 13 Oct 2019 17:42:02 +0200
Subject: =?UTF-8?q?Lade=20till=20text=20p=C3=A5=20off-circuit.tex?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 Dokument/Designspec/events/off-circuit.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'Dokument/Designspec/events/off-circuit.tex')

diff --git a/Dokument/Designspec/events/off-circuit.tex b/Dokument/Designspec/events/off-circuit.tex
index 3f11903..6c242cf 100644
--- a/Dokument/Designspec/events/off-circuit.tex
+++ b/Dokument/Designspec/events/off-circuit.tex
@@ -1,5 +1,5 @@
 Systemet ska detektera att en bil har åkt av banan inom 10 sekunder. Om systemet
 inte får en ny givarsignal inom tio sekunder från den senaste givaren antas bilen ha
 fastnat eller åkt av banan och programmet pausas tills bilen är på banan igen
-och användaren trycker på ``fortsätt'' på displayen.
+och användaren trycker på "fortsätt" på displayen. Med givarnas förväntade tidspassering så ska programmet kunna se att en bil inte passerat en givare vid den förväntade tidspasseringen. Har bilen inte passerat någon av givarna inom fem sekunder så kan programmet öka spänningsnivån gradvis som vid start för att kontrollera om bilen har stannat. Om ingen givare ger utslag inom fem sekunder till så ska programmet pausas och displayen skriva ut att det gjort det.
 
-- 
cgit v1.2.1

