From 294c6bf20787d2c751f323ef7152a14b5432e20d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Gustav=20S=C3=B6rn=C3=A4s?= <gusso230@student.liu.se>
Date: Tue, 15 Oct 2019 12:01:29 +0200
Subject: =?UTF-8?q?Spr=C3=A5k=20och=20stavning?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 Dokument/Designspec/events/start.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'Dokument/Designspec/events/start.tex')

diff --git a/Dokument/Designspec/events/start.tex b/Dokument/Designspec/events/start.tex
index 98af554..6f2defc 100644
--- a/Dokument/Designspec/events/start.tex
+++ b/Dokument/Designspec/events/start.tex
@@ -1,7 +1,7 @@
 Vid start ska systemet hitta en spänningsnivå tillräckligt hög för att bilen ska
 börja rulla men inte så hög att den åker av banan i första kurvan. I början ska
 därför spänningen öka lite i taget tills bilen passerat målgivaren. När bilen
-passerat målgivaren bibehålls spänningsnivån tills nästa givaren passeras.
+passerat målgivaren bibehålls spänningsnivån tills nästa givare passeras.
 Då kan programmet göra beräkningar för en inledande konstant för bilen och
 det vanliga systemet kan ta vid och kontrollera bilens förväntade position mot
 dess uträknade position.
-- 
cgit v1.2.1

