From bf1d7fbea7379613c689167903da66ff2dea69d3 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Gustav=20S=C3=B6rn=C3=A4s?= <gusso230@student.liu.se>
Date: Tue, 8 Oct 2019 16:53:36 +0200
Subject: =?UTF-8?q?Spr=C3=A5k=20-=20start?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 Dokument/Designspec/events/start.tex | 9 +++++----
 1 file changed, 5 insertions(+), 4 deletions(-)

(limited to 'Dokument/Designspec/events/start.tex')

diff --git a/Dokument/Designspec/events/start.tex b/Dokument/Designspec/events/start.tex
index 4f0f30c..1476186 100644
--- a/Dokument/Designspec/events/start.tex
+++ b/Dokument/Designspec/events/start.tex
@@ -1,4 +1,5 @@
-Innan målgivaren hittar vi ett läge där alla bilar är körbara och inte fastnar.
-Till första givaren behåller bilen den spänning den behövde för att börja rulla
-och vi kan därefter veta hur lång tid det tagit mellan start och och första
-givaren. Med det kan vi räkna ut vilket vilken konstant (k) som bilen behöver. 
+För att systemet ska hitta en spänning som gör att bilen börjar rulla men inte
+åker av banan i första kurvan ökas spänningen i början lite i taget tills bilen
+passerar den första givaren. Efter det tar det vanliga systemet vid och
+kontrollerar bilens förväntade position mot dess uträknade position.
+
-- 
cgit v1.2.1

