From 646d1bb2c68b628a149c78fbd94a734943d3c252 Mon Sep 17 00:00:00 2001
From: Alexander Tuneskog <aletu130@student.liu.se>
Date: Mon, 2 Dec 2019 14:20:24 +0100
Subject: =?UTF-8?q?=C3=A4ndrade=20stavfel?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 Dokument/Teknisk Dokumentation/text/04-events.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'Dokument/Teknisk Dokumentation/text/04-events.tex')

diff --git a/Dokument/Teknisk Dokumentation/text/04-events.tex b/Dokument/Teknisk Dokumentation/text/04-events.tex
index 6f72713..5bb0052 100644
--- a/Dokument/Teknisk Dokumentation/text/04-events.tex	
+++ b/Dokument/Teknisk Dokumentation/text/04-events.tex	
@@ -3,8 +3,8 @@
 
 Programmet gör redan en uppskattning av bilens position (\texttt{get\_position()})
  och justerar denna vid ny givare, se \ref{sec:system:korning:position}.
-Eftersom \texttt{get\_new\_v()} utgår ifrån denna uppskattning, kommer ingen
-anpassning behöva göras ifall en givare inte ger utslag. Däremot måste det 
+Eftersom \texttt{get\_new\_v()} utgår ifrån denna uppskattning, behövs ingen
+anpassning göras ifall en givare inte ger utslag. Däremot måste det 
 kompenseras nästa gång en givare detekteras. Detta görs med funktionen
 \texttt{choose\_position()}. Den funktionen jämför positionen beräknad av 
 \texttt{get\_position()} och positionen vald av nuvarande givare. 
-- 
cgit v1.2.1

