From c0616c2e752b2c786b89a3aa84d185b970ae042e Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Gustav=20S=C3=B6rn=C3=A4s?= <gusso230@student.liu.se>
Date: Sun, 1 Dec 2019 15:49:28 +0100
Subject: =?UTF-8?q?Gustavs=20=C3=A4ndringar?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 Dokument/Teknisk Dokumentation/text/system/05-display.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'Dokument/Teknisk Dokumentation/text/system/05-display.tex')

diff --git a/Dokument/Teknisk Dokumentation/text/system/05-display.tex b/Dokument/Teknisk Dokumentation/text/system/05-display.tex
index f1baef2..9813e60 100644
--- a/Dokument/Teknisk Dokumentation/text/system/05-display.tex	
+++ b/Dokument/Teknisk Dokumentation/text/system/05-display.tex	
@@ -1,6 +1,6 @@
 \subsubsection{Display}
 
-I varje programcykel skickas nuvarande värdet på u till två stapeldiagram på
-displayen för vardera bil. Se appendix N för mer information om displayens
-stapeldiagram. Om ett nytt varv har inletts skrivs dessutom varvnumret och
+I varje programcykel skickas värdet på \texttt{car.u} till två stapeldiagram på
+displayen för vardera bil. Se REF för information om displayens
+stapeldiagram. Om ett nytt varv inleds skrivs dessutom förra varvnumret och
 varvtiden ut på displayen.
-- 
cgit v1.2.1

