From 10a69ab9418ea79142b7f6f83d80bccde60768f5 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?David=20Thor=C3=A9n?= <davth346@student.liu.se>
Date: Tue, 8 Oct 2019 15:17:56 +0200
Subject: =?UTF-8?q?Underrubriker=20till=20"HANTERING=20AV=20H=C3=84NDELSER?=
 =?UTF-8?q?"?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 Dokument/Designspec/events.tex | 7 +++++++
 1 file changed, 7 insertions(+)

(limited to 'Dokument/Designspec/events.tex')

diff --git a/Dokument/Designspec/events.tex b/Dokument/Designspec/events.tex
index 0728acd..32390a6 100644
--- a/Dokument/Designspec/events.tex
+++ b/Dokument/Designspec/events.tex
@@ -1,7 +1,14 @@
 \section{Hantering av händelser}
 
 \input{events/start}
+\section{Start}
 \input{events/off-circuit}
+\section{Avåkning}
+
 \input{events/missade-givare}
+\section{Missade givare}
+
 Enligt krav 3 i kravspecifikationen ska programmet kunna hantera missade givare och fortsätta köra som normalt. Som vi har tänkt att använda oss av givarna så ska inte bilarna ändra sin körning vid ett sådant utfall. Då vi tänkt att använda givarna som en referens och inte justering av bilarnas körning så kommer en missad givare ge ett fel på referens.
+
 \input{events/manuell}
+\section{Manuell körning}
-- 
cgit v1.2.1

